**talento smart B15 (basic)**

**Digital distributor time switch, 1 channel, integrated Bluetooth, programming by app, 2TE**

Digital distributor time switch with integrated Bluetooth interface and straightforward programming on the device, via the app or on a PC. No additional hardware required for program transfer. Protection against tampering provided by encrypted data transmission, PIN protection and product’s ability to be sealed. Daily, weekly and annual programs with 100 freely combinable switch commands. Shortest switching time 1 minute.

Supply voltage 110–230 V, 50–60 Hz; switching capacity: 1 potential-free changeover contact with zero crossing detection 16 A/250 V AC; 600 W LED load; 8 years’ power reserve; captive screw terminal with wire protection max. 2.5 mm²; high-resolution dot-matrix display with background lighting; automatic operation, fix ON/OFF, override;

Dimensions: 90 x 35.5 x 60 mm (H x W x D)

Manufacturer: Grässlin

Model: talento smart B15

Item no.: 43.02.0001.1